**NEW PILOT-OPERATED REGULATOR IN THE SYNTESI SERIES**

The range of Syntesi pressure regulators is complemented by the entry of the new pilot-operated version in the sizes Sy 1 and Sy2.

Ideal for use in all applications where pneumatically operated remote control is required, this new regulator can be operated by a double-diaphragm piston that ensures optimal flow rate, quick response and accurate regulation.

The new pilot-operated version is based on the same design as the Syntesi hand-operated regulator and offers the same advantages, i.e. the pressure offsetting that is regulated with the change in upstream pressure, the presence of a relieving valve and the quick discharge of downstream pressure.



Fig. 1 – The new pilot-operated regulator in the Syntesi series.

Corrado Tamiozzo, engineer

R&D Manager

Metal Work S.p.A.